IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView]"
File name: "7. Toit incliné mur - hellend dak wand.ifc"
Time stamp: "2021-01-26T16:37:05+01:00"
Preprocessor: "IfcOpenShell 0.6.0b0"
Originating system: "BlenderBIM 0.0.201025"
Authorization: "Nobody"

Units
  LENGTHUNIT: CENTI METRE
  AREAUNIT: CENTI SQUARE_METRE
  VOLUMEUNIT: CENTI CUBIC_METRE

Spatial structure
IFCPROJECT | long name "Projet"
  IFCSITE "Default" | postal address OFFICE
    IFCBUILDING "Default" | postal address OFFICE
      IFCBUILDINGSTOREY "1"
        contains 13 elements
          1 x IFCCOVERING | INSULATION | names: "Isolation - isolatie" | material: "Isolant souple de toiture" | property sets: Pset_CoveringCommon, Cpset_Covering, Qto_CoveringBaseQuantities
          1 x IFCPIPESEGMENT | GUTTER | names: "Gouttière - hanggoot" | material: "Zinc VMZINC - couleur zinc naturel"
          2 x IFCCOVERING | MEMBRANE | names: "Pare-vapeur - dampscherm", "Sous-toiture - onderdak" | material: "Membrane Pare vapeur"; "Membrane étanche" | property sets: Pset_CoveringCommon, Cpset_Covering, Qto_CoveringBaseQuantities
          1 x IFCCOVERING | CEILING | names: "Enduit - bepleistering" | material: "Enduit cimenté blanc" | property sets: Pset_CoveringCommon, Cpset_Covering, Qto_CoveringBaseQuantities, Cpset_Ceiling
          6 x IFCMEMBER | RAFTER | names: "Ferme - spanten" | material: "Bois - Pin" | property sets: Pset_MemberCommon, Cpset_Member
          1 x IFCPLATE | object type "Battens" | USERDEFINED | names: "(contre)lattage - pan- en tengellatten" | material: "Bois Contrelattage" | property sets: Pset_PlateCommon, Cpset_Plate
          1 x IFCCOVERING | ROOFING | names: "Couverture de toiture - dakbedekking" | material: "Tuiles ondulées - terre cuite" | property sets: Pset_CoveringCommon, Cpset_Covering, Qto_CoveringBaseQuantities
      IFCBUILDINGSTOREY "0"
        contains 8 elements
          1 x IFCBEAM | BEAM | names: "Poutre de ceinture - ringbalk" | material: "Béton coulé" | property sets: Pset_BeamCommon, Cpset_Beam, Cpset_ConcreteElementGeneral, Cpset_PrecastConcreteElement, Qto_BeamBaseQuantities
          1 x IFCCOVERING | INSULATION | names: "Isolation - spouwisolatie" | material: "Isolant rigide de mur" | property sets: Pset_CoveringCommon, Cpset_Covering, Qto_CoveringBaseQuantities
          1 x IFCWALL | SOLIDWALL | names: "Maçonnerie portante - binnenspouwblad" | material: "Bloc béton - 14 cm" | property sets: Pset_WallCommon, Cpset_Wall, Cpset_PrecastConcreteElement, Cpset_ConcreteElementGeneral, Qto_WallBaseQuantities
          1 x IFCPIPESEGMENT | RIGIDSEGMENT | names: "Descente d'eau de pluie - afvoerpijpen" | material: "Zinc VMZINC - couleur zinc naturel"
          2 x IFCCOVERING | CLADDING | names: "Enduit - bepleistering", "Briques de parement - gevelmetselwerk" | material: "Enduit cimenté blanc"; "Briques" | property sets: Pset_CoveringCommon, Cpset_Covering, Qto_CoveringBaseQuantities
          1 x IFCMEMBER | PLATE | names: "Sablière - muurplaat" | material: "Bois - Pin" | property sets: Pset_MemberCommon, Cpset_Member
          1 x IFCDISCRETEACCESSORY | object type "Edge fixing plate" | USERDEFINED | names: "Planche de rive - boordplank" | material: "blanc"

Property sets
  Pset_CoveringCommon | properties | on 8 objects (8 IFCCOVERING)
    Finish = "x" (IFCTEXT)
    FireRating = "x" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "x" (IFCIDENTIFIER)
    Status = "x" (IFCTEXT)
  Cpset_Covering | properties | on 8 objects (8 IFCCOVERING)
    PRReactionToFire = "x" (IFCLABEL)
    PRSoundReductionIndex = "x" (IFCLABEL)
    PRThermalConductivity = 0. (IFCTHERMALCONDUCTIVITYMEASURE)
    PRThermalResistance = 0. (IFCTHERMALRESISTANCEMEASURE)
    Phasing = "x" (IFCLABEL)
  Qto_CoveringBaseQuantities | quantities | on 8 objects (8 IFCCOVERING)
    GrossArea = 0. [CENTI SQUARE_METRE]
    NetArea = 0. [CENTI SQUARE_METRE]
    Width = 0. [CENTI METRE]
  Cpset_Ceiling | properties | on 1 object (1 IFCCOVERING)
    ClimateCeiling = TRUE (IFCBOOLEAN)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    FireRating = "x" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "x" (IFCIDENTIFIER)
    Status = "x" (IFCTEXT)
  Cpset_Wall | properties | on 1 object (1 IFCWALL)
    ExternalSurfaceTreatment = "x" (IFCLABEL)
    PRReactionToFire = "x" (IFCLABEL)
    PRSoundReductionIndex = "x" (IFCLABEL)
    PRThermalConductivity = 0. (IFCTHERMALCONDUCTIVITYMEASURE)
    PRThermalResistance = 0. (IFCTHERMALRESISTANCEMEASURE)
    Phasing = "x" (IFCLABEL)
    SurfaceCharacteristics = "x" (IFCLABEL)
  Cpset_PrecastConcreteElement | properties | on 2 objects (1 IFCBEAM, 1 IFCWALL)
    CornerChamfer = 0. (IFCLENGTHMEASURE) [CENTI METRE]
  Cpset_ConcreteElementGeneral | properties | on 2 objects (1 IFCBEAM, 1 IFCWALL)
    ConstructionMethod = "x" (IFCLABEL)
    ReinforcementVolumeRatio = 0. (IFCMASSDENSITYMEASURE)
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossVolume = 0. [CENTI CUBIC_METRE]
    Height = 0. [CENTI METRE]
    Length = 0. [CENTI METRE]
    NetSideArea = 0. [CENTI SQUARE_METRE]
    NetVolume = 0. [CENTI CUBIC_METRE]
    Width = 0. [CENTI METRE]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    FireRating = "x" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "x" (IFCIDENTIFIER)
    Status = "x" (IFCTEXT)
  Cpset_Beam | properties | on 1 object (1 IFCBEAM)
    ExternalSurfaceTreatment = "x" (IFCLABEL)
    PRReactionToFire = "x" (IFCLABEL)
    PRSoundReductionIndex = "x" (IFCLABEL)
    PRThermalConductivity = 0. (IFCTHERMALCONDUCTIVITYMEASURE)
    PRThermalResistance = 0. (IFCTHERMALRESISTANCEMEASURE)
    Phasing = "x" (IFCLABEL)
    SurfaceCharacteristics = "x" (IFCLABEL)
  Qto_BeamBaseQuantities | quantities | on 1 object (1 IFCBEAM)
    CrossSectionArea = 0. [CENTI SQUARE_METRE]
    GrossVolume = 0. [CENTI CUBIC_METRE]
    Length = 0. [CENTI METRE]
    NetVolume = 0. [CENTI CUBIC_METRE]
    OuterSurfaceArea = 0. [CENTI SQUARE_METRE]
  Pset_MemberCommon | properties | on 7 objects (7 IFCMEMBER)
    FireRating = "x" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "x" (IFCIDENTIFIER)
    Status = "x" (IFCTEXT)
  Cpset_Member | properties | on 7 objects (7 IFCMEMBER)
    PRReactionToFire = "x" (IFCLABEL)
    PRSoundReductionIndex = "x" (IFCLABEL)
    PRThermalConductivity = 0. (IFCTHERMALCONDUCTIVITYMEASURE)
    PRThermalResistance = 0. (IFCTHERMALRESISTANCEMEASURE)
    Phasing = "x" (IFCLABEL)
  Pset_PlateCommon | properties | on 1 object (1 IFCPLATE)
    FireRating = "x" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "x" (IFCIDENTIFIER)
    Status = "x" (IFCTEXT)
  Cpset_Plate | properties | on 1 object (1 IFCPLATE)
    PRReactionToFire = "x" (IFCLABEL)
    PRSoundReductionIndex = "x" (IFCLABEL)
    PRThermalConductivity = 0. (IFCTHERMALCONDUCTIVITYMEASURE)
    PRThermalResistance = 0. (IFCTHERMALRESISTANCEMEASURE)
    Phasing = "x" (IFCLABEL)