IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView]"
File name: "6. Structure - Structuur.blend.ifc"
Time stamp: "2020-12-22T11:17:37+01:00"
Preprocessor: "IfcOpenShell 0.6.0b0"
Originating system: "BlenderBIM 0.0.200912"
Authorization: "Nobody"

Units
  LENGTHUNIT: CENTI METRE
  AREAUNIT: CENTI SQUARE_METRE
  VOLUMEUNIT: CENTI CUBIC_METRE

Spatial structure
IFCPROJECT | long name "Projet"
  IFCSITE "Default" | postal address OFFICE
    IFCBUILDING "Default" | postal address OFFICE
      IFCBUILDINGSTOREY "1"
        contains 4 elements
          2 x IFCBEAM | BEAM | names: "Poutre - balk" | material: "Béton coulé" | property sets: Pset_BeamCommon, Cpset_Beam, Cpset_ConcreteElementGeneral, Cpset_PrecastConcreteElement, Qto_BeamBaseQuantities
          2 x IFCSLAB | FLOOR | names: "Hourdis - welfsel", "Chape de compression - druklaag" | material: "Hourdis"; "Chape de compression" | property sets: Pset_SlabCommon, Cpset_Slab, Cpset_ConcreteElementGeneral, Cpset_PrecastConcreteElement, Qto_SlabBaseQuantities, Pset_PrecastSlab
      IFCBUILDINGSTOREY "0"
        contains 2 elements
          1 x IFCDISCRETEACCESSORY | USERDEFINED | names: "Matériau de connexion - oplegmateriaal" | material: "<Unnamed>"
          1 x IFCCOLUMN | COLUMN | names: "Colonne - kolom" | material: "Béton coulé" | property sets: Pset_ColumnCommon, Cpset_Column, Cpset_PrecastConcreteElement, Cpset_ConcreteElementGeneral, Qto_ColumnBaseQuantities

Property sets
  Pset_BeamCommon | properties | on 2 objects (2 IFCBEAM)
    FireRating = "x" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "x" (IFCIDENTIFIER)
    Status = "x" (IFCTEXT)
  Cpset_Beam | properties | on 2 objects (2 IFCBEAM)
    ExternalSurfaceTreatment = "x" (IFCLABEL)
    PRReactionToFire = "x" (IFCLABEL)
    PRSoundReductionIndex = "x" (IFCLABEL)
    PRThermalConductivity = 0. (IFCTHERMALCONDUCTIVITYMEASURE)
    PRThermalResistance = 0. (IFCTHERMALRESISTANCEMEASURE)
    Phasing = "x" (IFCLABEL)
    SurfaceCharacteristics = "x" (IFCLABEL)
  Cpset_ConcreteElementGeneral | properties | on 5 objects (2 IFCBEAM, 2 IFCSLAB, 1 IFCCOLUMN)
    ConstructionMethod = "x" (IFCLABEL)
    ReinforcementVolumeRatio = 0. (IFCMASSDENSITYMEASURE)
  Cpset_PrecastConcreteElement | properties | on 5 objects (2 IFCBEAM, 2 IFCSLAB, 1 IFCCOLUMN)
    CornerChamfer = 0. (IFCLENGTHMEASURE) [CENTI METRE]
  Qto_BeamBaseQuantities | quantities | on 2 objects (2 IFCBEAM)
    CrossSectionArea = 0. [CENTI SQUARE_METRE]
    GrossVolume = 0. [CENTI CUBIC_METRE]
    Length = 0. [CENTI METRE]
    NetVolume = 0. [CENTI CUBIC_METRE]
    OuterSurfaceArea = 0. [CENTI SQUARE_METRE]
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    FireRating = "x" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "x" (IFCIDENTIFIER)
    Status = "x" (IFCTEXT)
  Cpset_Slab | properties | on 2 objects (2 IFCSLAB)
    ExternalSurfaceTreatment = "x" (IFCLABEL)
    PRReactionToFire = "x" (IFCLABEL)
    PRSoundReductionIndex = "x" (IFCLABEL)
    PRThermalConductivity = 0. (IFCTHERMALCONDUCTIVITYMEASURE)
    PRThermalResistance = 0. (IFCTHERMALRESISTANCEMEASURE)
    Phasing = "x" (IFCLABEL)
    SurfaceCharacteristics = "x" (IFCLABEL)
  Qto_SlabBaseQuantities | quantities | on 2 objects (2 IFCSLAB)
    Depth = 0. [CENTI METRE]
    GrossArea = 0. [CENTI SQUARE_METRE]
    GrossVolume = 0. [CENTI CUBIC_METRE]
    Length = 0. [CENTI METRE]
    NetArea = 0. [CENTI SQUARE_METRE]
    NetVolume = 0. [CENTI CUBIC_METRE]
    Perimeter = 0. [CENTI METRE]
    Width = 0. [CENTI METRE]
  Pset_PrecastSlab | properties | on 2 objects (2 IFCSLAB)
    TypeDesignator = "x" (IFCLABEL)
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    FireRating = "x" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "x" (IFCIDENTIFIER)
    Status = "x" (IFCTEXT)
  Cpset_Column | properties | on 1 object (1 IFCCOLUMN)
    ExternalSurfaceTreatment = "x" (IFCLABEL)
    PRReactionToFire = "x" (IFCLABEL)
    PRSoundReductionIndex = "x" (IFCLABEL)
    PRThermalConductivity = 0. (IFCTHERMALCONDUCTIVITYMEASURE)
    PRThermalResistance = 0. (IFCTHERMALRESISTANCEMEASURE)
    Phasing = "x" (IFCLABEL)
    SurfaceCharacteristics = "x" (IFCLABEL)
  Qto_ColumnBaseQuantities | quantities | on 1 object (1 IFCCOLUMN)
    CrossSectionArea = 0. [CENTI SQUARE_METRE]
    GrossVolume = 0. [CENTI CUBIC_METRE]
    Length = 0. [CENTI METRE]
    NetVolume = 0. [CENTI CUBIC_METRE]
    OuterSurfaceArea = 0. [CENTI SQUARE_METRE]